# transport.h File Reference

`#include <jack/types.h>`

Go to the source code of this file.

## Data Structures
struct | jack_position_t
struct | jack_transport_info_t
## Defines
#define | JACK_POSITION_MASK (JackPositionBBT|JackPositionTimecode|JackBBTFrameOffset|JackAudioVideoRatio|JackVideoFrameOffset)
#define | EXTENDED_TIME_INFO
## Typedefs
typedef uint64_t | jack_unique_t
typedef int(* | JackSyncCallback )(jack_transport_state_t state, jack_position_t *pos, void *arg)
typedef void(* | JackTimebaseCallback )(jack_transport_state_t state, jack_nframes_t nframes, jack_position_t *pos, int new_pos, void *arg)
## Enumerations
enum | jack_transport_state_t { JackTransportStopped = 0, JackTransportRolling = 1, JackTransportLooping = 2, JackTransportStarting = 3 }
enum | jack_position_bits_t { JackPositionBBT = 0x10, JackPositionTimecode = 0x20, JackBBTFrameOffset = 0x40, JackAudioVideoRatio = 0x80, JackVideoFrameOffset = 0x100 }
enum | jack_transport_bits_t { JackTransportState = 0x1, JackTransportPosition = 0x2, JackTransportLoop = 0x4, JackTransportSMPTE = 0x8, JackTransportBBT = 0x10 }
## Functions
int | jack_release_timebase (jack_client_t *client)
int | jack_set_sync_callback (jack_client_t *client, JackSyncCallback sync_callback, void *arg)
int | jack_set_sync_timeout (jack_client_t *client, jack_time_t timeout)
int | jack_set_timebase_callback (jack_client_t *client, int conditional, JackTimebaseCallback timebase_callback, void *arg)
int | jack_transport_locate (jack_client_t *client, jack_nframes_t frame)
jack_transport_state_t | jack_transport_query (const jack_client_t *client, jack_position_t *pos)
jack_nframes_t | jack_get_current_transport_frame (const jack_client_t *client)
int | jack_transport_reposition (jack_client_t *client, jack_position_t *pos)
void | jack_transport_start (jack_client_t *client)
void | jack_transport_stop (jack_client_t *client)
void | jack_get_transport_info (jack_client_t *client, jack_transport_info_t *tinfo)
void | jack_set_transport_info (jack_client_t *client, jack_transport_info_t *tinfo)

## Define Documentation

#define EXTENDED_TIME_INFO

#define JACK_POSITION_MASK (JackPositionBBT|JackPositionTimecode|JackBBTFrameOffset|JackAudioVideoRatio|JackVideoFrameOffset)

| all valid position bits

## Typedef Documentation

typedef uint64_t jack_unique_t

| Unique ID (opaque)

typedef int(* JackSyncCallback)(jack_transport_state_t state, jack_position_t *pos, void *arg)

  | Prototype for the sync_callback defined by slow-sync clients. When the client is active, this callback is invoked just before process() in the same thread. This occurs once after registration, then subsequently whenever some client requests a new position, or the transport enters the JackTransportStarting state. This realtime function must not wait. The transport state will be: JackTransportStopped when a new position is requested; JackTransportStarting when the transport is waiting to start; JackTransportRolling when the timeout has expired, and the position is now a moving target. Parameters:
  | state | current transport state.
  | pos | new transport position.
  | arg | the argument supplied by jack_set_sync_callback().
Returns: TRUE (non-zero) when ready to roll.

typedef void(* JackTimebaseCallback)(jack_transport_state_t state, jack_nframes_t nframes, jack_position_t *pos, int new_pos, void *arg)

  | Prototype for the timebase_callback used to provide extended position information. Its output affects all of the following process cycle. This realtime function must not wait. This function is called immediately after process() in the same thread whenever the transport is rolling, or when any client has requested a new position in the previous cycle. The first cycle after jack_set_timebase_callback() is also treated as a new position, or the first cycle after jack_activate() if the client had been inactive. The timebase master may not use its pos argument to set pos->frame. To change position, use jack_transport_reposition() or jack_transport_locate(). These functions are realtime-safe, the timebase_callback can call them directly. Parameters:
  | state | current transport state.
  | nframes | number of frames in current period.
  | pos | address of the position structure for the next cycle; pos->frame will be its frame number. If new_pos is FALSE, this structure contains extended position information from the current cycle. If TRUE, it contains whatever was set by the requester. The timebase_callback's task is to update the extended information here.
  | new_pos | TRUE (non-zero) for a newly requested pos, or for the first cycle after the timebase_callback is defined.
  | arg | the argument supplied by jack_set_timebase_callback().

## Enumeration Type Documentation

enum jack_position_bits_t

  | Optional struct jack_position_t fields. Enumerator:
  JackPositionBBT | Bar, Beat, Tick
  JackPositionTimecode | External timecode
  JackBBTFrameOffset | Frame offset of BBT information
  JackAudioVideoRatio | audio frames per video frame
  JackVideoFrameOffset | frame offset of first video frame

enum jack_transport_bits_t

  | Optional struct jack_transport_info_t fields. See also: jack_position_bits_t. Enumerator:
  JackTransportState | Transport state
  JackTransportPosition | Frame number
  JackTransportLoop | Loop boundaries (ignored)
  JackTransportSMPTE | SMPTE (ignored)
  JackTransportBBT | Bar, Beat, Tick

enum jack_transport_state_t

  | Transport states. Enumerator:
  JackTransportStopped | Transport halted
  JackTransportRolling | Transport playing
  JackTransportLooping | For OLD_TRANSPORT, now ignored
  JackTransportStarting | Waiting for sync ready

## Function Documentation

jack_nframes_t jack_get_current_transport_frame | ( | const jack_client_t * | client | ) |

  | Return an estimate of the current transport frame, including any time elapsed since the last transport positional update. Parameters:
  | client | the JACK client structure

void jack_get_transport_info | ( | jack_client_t * | client,
|  | jack_transport_info_t * | tinfo
| ) |

  | Gets the current transport info structure (deprecated). Parameters:
  | client | the JACK client structure.
  | tinfo | current transport info structure. The "valid" field describes which fields contain valid data.
Deprecated: This is for compatibility with the earlier transport interface. Use jack_transport_query(), instead. Precondition: Must be called from the process thread.

int jack_release_timebase | ( | jack_client_t * | client | ) |

  | Called by the timebase master to release itself from that responsibility. If the timebase master releases the timebase or leaves the JACK graph for any reason, the JACK engine takes over at the start of the next process cycle. The transport state does not change. If rolling, it continues to play, with frame numbers as the only available position information. See also: jack_set_timebase_callback Parameters:
  | client | the JACK client structure.
Returns: 0 on success, otherwise a non-zero error code.

int jack_set_sync_callback | ( | jack_client_t * | client,
|  | JackSyncCallback | sync_callback,
|  | void * | arg
| ) |

  | Register (or unregister) as a slow-sync client, one that cannot respond immediately to transport position changes. The sync_callback will be invoked at the first available opportunity after its registration is complete. If the client is currently active this will be the following process cycle, otherwise it will be the first cycle after calling jack_activate(). After that, it runs according to the JackSyncCallback rules. Clients that don't set a sync_callback are assumed to be ready immediately any time the transport wants to start. Parameters:
  | client | the JACK client structure.
  | sync_callback | is a realtime function that returns TRUE when the client is ready. Setting sync_callback to NULL declares that this client no longer requires slow-sync processing.
  | arg | an argument for the sync_callback function.
Returns: 0 on success, otherwise a non-zero error code.

int jack_set_sync_timeout | ( | jack_client_t * | client,
|  | jack_time_t | timeout
| ) |

  | Set the timeout value for slow-sync clients. This timeout prevents unresponsive slow-sync clients from completely halting the transport mechanism. The default is two seconds. When the timeout expires, the transport starts rolling, even if some slow-sync clients are still unready. The sync_callbacks of these clients continue being invoked, giving them a chance to catch up. See also: jack_set_sync_callback Parameters:
  | client | the JACK client structure.
  | timeout | is delay (in microseconds) before the timeout expires.
Returns: 0 on success, otherwise a non-zero error code.

int jack_set_timebase_callback | ( | jack_client_t * | client,
|  | int | conditional,
|  | JackTimebaseCallback | timebase_callback,
|  | void * | arg
| ) |

  | Register as timebase master for the JACK subsystem. The timebase master registers a callback that updates extended position information such as beats or timecode whenever necessary. Without this extended information, there is no need for this function. There is never more than one master at a time. When a new client takes over, the former timebase_callback is no longer called. Taking over the timebase may be done conditionally, so it fails if there was a master already. Parameters:
  | client | the JACK client structure.
  | conditional | non-zero for a conditional request.
  | timebase_callback | is a realtime function that returns position information.
  | arg | an argument for the timebase_callback function.
Returns: 0 on success; EBUSY if a conditional request fails because there was already a timebase master; other non-zero error code.

void jack_set_transport_info | ( | jack_client_t * | client,
|  | jack_transport_info_t * | tinfo
| ) |

| Set the transport info structure (deprecated). Deprecated: This function still exists for compatibility with the earlier transport interface, but it does nothing. Instead, define a JackTimebaseCallback.

int jack_transport_locate | ( | jack_client_t * | client,
|  | jack_nframes_t | frame
| ) |

  | Reposition the transport to a new frame number. May be called at any time by any client. The new position takes effect in two process cycles. If there are slow-sync clients and the transport is already rolling, it will enter the JackTransportStarting state and begin invoking their sync_callbacks until ready. This function is realtime-safe. See also: jack_transport_reposition, jack_set_sync_callback Parameters:
  | client | the JACK client structure.
  | frame | frame number of new transport position.
Returns: 0 if valid request, non-zero otherwise.

jack_transport_state_t jack_transport_query | ( | const jack_client_t * | client,
|  | jack_position_t * | pos
| ) |

  | Query the current transport state and position. This function is realtime-safe, and can be called from any thread. If called from the process thread, pos corresponds to the first frame of the current cycle and the state returned is valid for the entire cycle. Parameters:
  | client | the JACK client structure.
  | pos | pointer to structure for returning current transport position; pos->valid will show which fields contain valid data. If pos is NULL, do not return position information.
Returns: Current transport state.

int jack_transport_reposition | ( | jack_client_t * | client,
|  | jack_position_t * | pos
| ) |

  | Request a new transport position. May be called at any time by any client. The new position takes effect in two process cycles. If there are slow-sync clients and the transport is already rolling, it will enter the JackTransportStarting state and begin invoking their sync_callbacks until ready. This function is realtime-safe. See also: jack_transport_locate, jack_set_sync_callback Parameters:
  | client | the JACK client structure.
  | pos | requested new transport position.
Returns: 0 if valid request, EINVAL if position structure rejected.

void jack_transport_start | ( | jack_client_t * | client | ) |

  | Start the JACK transport rolling. Any client can make this request at any time. It takes effect no sooner than the next process cycle, perhaps later if there are slow-sync clients. This function is realtime-safe. See also: jack_set_sync_callback Parameters:
  | client | the JACK client structure.

void jack_transport_stop | ( | jack_client_t * | client | ) |

  | Stop the JACK transport. Any client can make this request at any time. It takes effect on the next process cycle. This function is realtime-safe. Parameters:
  | client | the JACK client structure.